EANCOM PART II |  | 1997-07-01

CONTRL | - | Control message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 5 |  | Next Segment

SG1 | - | C | 999999 | - | UCM-SG2
SG2 | - | C | 999 | - | UCS-UCD
UCD | - | C | 99 | - | DATA ELEMENT ERROR INDICATOR
Function:
To identify an erroreous simple, composite or component data element, and to identify the nature of the error.
EDIFACT
EAN
*
Description |
0085
Syntax error, coded
M |  | an..3
M
*
12 = Invalid value
13 = Missing
14 = Value not supported in this position
15 = Not supported in this position
16 = Too many constituents
18 = Unspecified error
19 = Invalid decimal notation
21 = Invalid character(s)
22 = Invalid service character(s)
27 = Security function not supported
34 = Nesting indicator not allowed
37 = Invalid type of character(s)
38 = Missing digit in front of decimal sign
39 = Data element too long
40 = Data element too short
S011
DATA ELEMENT POSITION
M |
M
| 0098
| Erroneous data element position in segment |
M |  | n..3
M
| 0104
| Erroneous component data element position |
C |  | n..3
O
Segment Notes:
This segment is used to identify the position of a component or composite data element within a segment. This segment is only used to identify component or composite data elements within the segment identified in the UCS segment which have errors. DE 0098: The numerical count position of the simple or composite data element in error. The segment tag and each simple and composite data element position number within the segment. DE 0104: The numerical count position of the component data element in error. Each component data element position defined in the composite data element description shall cause the count to be incremented. Example : UCD+12+4:4'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |