EANCOM PART II |  | 1997-07-01

INVRPT | - | Inventory report message | VERSION | 004

5. Segments Layout |

Previous Segment |  | Segment number: | 17 |  | Next Segment

SG9 | - | C | 9999 | - | LIN-PIA-IMD-SG11
SG11 | - | C | 9999 | - | QTY-INV-GIN-LOC-DTM-STS-SG13-SG14-SG15
GIN | - | C | 9999 | - | Goods identity number
Function:
To give specific identification numbers, either as single numbers or ranges.
EDIFACT
EAN
*
Description |
7405
Identity number qualifier
M |  | an..3
M
*
BN = Serial number
BX = Batch number
C208
IDENTITY NUMBER RANGE
M |
M
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
Segment Notes:
This segment is used to provide additional identification numbers relevant to the line item identified in the LIN segment and specific to the quantities reported in the QTY segment. EAN/UCC Serial Shipping Container Codes (SSCC) are provided in the GIN segment in the CPS segment group. DE C208: If a sequential series of identity numbers is provided (e.g., from 1 up to and including 10) only one repetition of composite C208 is needed with the first repetition of 7402 specifying the smaller number (e.g., 1) and the second repetition the larger number (e.g., 10). If the identity numbers are not sequential and part of a series (e.g., 1, 3, and 10) then a separate C208 and DE 7402 must be used for each identity number. Example : GIN+BX+456:500' This example defines a range of batch numbers from 456 to 500 inclusive.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |