EANCOM PART II |  | 1997-07-01

CONTRL | - | Control message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 4 |  | Next Segment

SG1 | - | C | 999999 | - | UCM-SG2
SG2 | - | C | 999 | - | UCS-UCD
UCS | - | M | 1 | - | SEGMENT ERROR INDICATION
Function:
To identify either a segment containing an error or a missing segment, and to identify any error related to the complete segment.
EDIFACT
EAN
*
Description |
0096
Segment position in message
M |  | n..6
M
0085
Syntax error, coded
C |  | an..3
O
*
12 = Invalid value
13 = Missing
14 = Value not supported in this position
15 = Not supported in this position
16 = Too many constituents
18 = Unspecified error
21 = Invalid character(s)
22 = Invalid service character(s)
27 = Security function not supported
34 = Nesting indicator not allowed
35 = Too many segment repetitions
36 = Too many segment group repetitions
Segment Notes:
This segment is used to identify the position of a segment within a message. This segment is only used to identify segments within the message identified in the UCM segment which have errors. DE 0085: This data element may be used to identify an error related to the complete segment. DE 0096: The numerical count position of a specific segment that is within the received message. The numbering starts with, and includes, the UNH segment as segment number 1. To identify a segment that contains an error, use the numerical count position of that segment. To report that a segment that is missing use the numerical count position of the last segment that was processed prior to the position where the missing segment was expected to be. A missing segment group is denoted by identifying the first segment in the group as missing. Example : UCS+3+12'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |