EANCOM PART II |  | 1997-07-01

DESADV | - | Despatch advice message | VERSION | 005

5. Segments Layout |

Previous Segment |  | Segment number: | 22 |  | Next Segment

SG10 | - | C | 9999 | - | CPS-SG11-SG15
SG11 | - | C | 9999 | - | PAC-MEA-QTY-SG12-SG13
SG13 | - | C | 1000 | - | PCI-RFF-DTM-SG14
PCI | - | M | 1 | - | Package identification
Function:
To specify markings and labels on individual packages or physical units.
EDIFACT
EAN
*
Description |
4233
Marking instructions, coded
C |  | an..3
R
33E = Marked with serial shipping container code (EAN Code)
C210
MARKS & LABELS
C |
O
| 7102
| Shipping marks |
M |  | an..35
M
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
8275
Container/package status, coded
C |  | an..3
N
C827
TYPE OF MARKING
C |
N
| 7511
| Type of marking, coded |
M |  | an..3
| 1131
| Code list qualifier |
C |  | an..3
| 3055
| Code list responsible agency, coded |
C |  | an..3
Segment Notes:
This segment is used to provide markings and labels information relevant to the packaging unit and level identified in the PAC segment. Example : PCI+33E'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |