EANCOM PART II |  | 1997-07-01

IFCSUM | - | Forwarding and consolidation summary message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 42 |  | Next Segment

SG15 | - | C | 9999 | - | CNI-DTM-CNT-TSR-MOA-FTX-SG21-SG22-SG30-SG37-SG56
SG37 | - | C | 999 | - | GID-HAN-TMP-RNG-MOA-PIA-FTX-SG38-SG39-SG40-SG41-SG42-SG43-SG48-SG51
RNG | - | C | 1 | - | Range details
Function:
To identify a range.
EDIFACT
EAN
*
Description |
6167
Range type qualifier
M |  | an..3
M
*
5 = Temperature range
C280
RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
CEL = Degree celsius
FAH = Degree fahrenheit
| 6162
| Range minimum |
C |  | n..18
R
| 6152
| Range maximum |
C |  | n..18
O
Segment Notes:
This segment is used to specify a temperature range for the current goods item. Example : RNG+5+CEL:40:45'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |