EANCOM PART II |  | 1997-07-01

IFCSUM | - | Forwarding and consolidation summary message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 58 |  | Next Segment

SG15 | - | C | 9999 | - | CNI-DTM-CNT-TSR-MOA-FTX-SG21-SG22-SG30-SG37-SG56
SG37 | - | C | 999 | - | GID-HAN-TMP-RNG-MOA-PIA-FTX-SG38-SG39-SG40-SG41-SG42-SG43-SG48-SG51
SG48 | - | C | 999 | - | SGP
SGP | - | M | 1 | - | Split goods placement
Function:
To specify the placement of goods in relation to equipment.
EDIFACT
EAN
*
Description |
C237
EQUIPMENT IDENTIFICATION
M |
M
| 8260
| Equipment identification number |
C |  | an..17
R
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
N
| 3207
| Country, coded |
C |  | an..3
O
ISO 3166 two alpha code |
7224
Number of packages
C |  | n..8
O
Segment Notes:
This segment is used to specify the placement of the goods item within the equipment used for its transportation. DE 8260: The value in DE 8260 indicates the identity number of the equipment in/on which the goods item is transported. Example : SGP+AS-12388'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |