EANCOM PART II |  | 1997-07-01

HANMOV | - | Cargo/goods handling and movement message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 14 |  | Next Segment

SG7 | - | C | 99 | - | LIN-PIA-IMD-HAN-SG8-QTY-DTM-FTX-SG10-SG11
HAN | - | C | 9 | - | Handling instructions
Function:
To specify handling and where necessary, notify hazards.
EDIFACT
EAN
*
Description |
C524
HANDLING INSTRUCTIONS
C |
R
| 4079
| Handling instructions, coded |
C |  | an..3
R
*
DES = Destroy (EAN Code)
LAB = Label (EAN Code)
MOV = Move (EAN Code)
PAC = Pack (EAN Code)
PFS = Prepare for shipment (EAN Code)
PIC = Pick (EAN Code)
PKS = Pick in sequence (EAN Code)
UNP = Unpack (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
R
*
9 = EAN (International Article Numbering association)
| 4078
| Handling instructions |
C |  | an..70
O
C218
HAZARDOUS MATERIAL
C |
O
| 7419
| Hazardous material class code, identification |
C |  | an..4
O
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
Segment Notes:
This segment is used to provide handling instructions, and where necessary to provide hazardous information, relevant to the current line item. Use of this segment at line level is not recommended if the HAN segment at heading level has been included. Users are recommended to indicate handling instructions at either heading or detail level but not both. DE 4079: When using the code PKS, Pick in sequence, the sequence in which the picking is to take place is specified by the sequence in which the LIN segments appear in the message. Example : HAN+LAB::9'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |