EANCOM PART II |  | 1997-07-01

RETANN | - | Returns announcement | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 32 |  | Next Segment

SG11 | - | C | 9999 | - | LIN-PIA-IMD-MEA-DTM-PRI-LOC-MOA-SG13-SG14-SG15-SG18-SG22
SG18 | - | C | 9 | - | PAC-SG19
SG19 | - | C | 9 | - | PCI-DTM-GIN
PCI | - | M | 9 | - | Package identification
Function:
To specify markings and labels on individual packages or physical units.
EDIFACT
EAN
*
Description |
4233
Marking instructions, coded
C |  | an..3
R
14 = Mark expiry date
16 = Buyer's instructions
17 = Supplier's instructions
33E = Marked with serial shipping container code (EAN Code)
34E = Marked with EAN/UPC number (EAN Code)
C210
MARKS & LABELS
C |
O
| 7102
| Shipping marks |
M |  | an..35
M
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
8275
Container/package status, coded
C |  | an..3
N
C827
TYPE OF MARKING
C |
N
| 7511
| Type of marking, coded |
M |  | an..3
| 1131
| Code list qualifier |
C |  | an..3
| 3055
| Code list responsible agency, coded |
C |  | an..3
Segment Notes:
This segment is used to provide markings and labels information relevant to the packaging unit identified in the PAC segment. This information may be used at the time of collection to correctly identify the packages for return. Example : PCI+33E'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |