EANCOM PART II |  | 1997-07-01

RECADV | - | Receiving advice message | VERSION | 003

5. Segments Layout |

Previous Segment |  | Segment number: | 13 |  | Next Segment

SG16 | - | C | 9999 | - | CPS-SG17-SG22
SG17 | - | C | 9999 | - | PAC-QVR-SG18
QVR | - | C | 1 | - | Quantity variances
Function:
To specify item details relating to quantity variances. Note: This segment replaces segment QVA (which has been deleted in this directory).
EDIFACT
EAN
*
Description |
C279
QUANTITY DIFFERENCE INFORMATION
C |
R
| 6064
| Quantity difference |
M |  | n..15
M
Specify the actual variance amount here. |
| 6063
| Quantity qualifier |
C |  | an..3
R
124 = Damaged goods
4221
Discrepancy, coded
C |  | an..3
O
C960
REASON FOR CHANGE
C |
O
| 4295
| Change reason, coded |
C |  | an..3
O
AUE = Article code unknown (EAN Code)
BN = Bar code not readable (EAN Code)
PC = Pack difference
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
9 = EAN (International Article Numbering association)
| 4294
| Change reason |
C |  | an..35
O
Segment Notes:
This segment is used to indicate quantity variances related to the currently identified package. For negative values (e.g. damaged goods not accepted) the variance must be expressed as negative. Example : QVR+-40:124++BN'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |