EANCOM PART II |  | 1997-07-01

IFCSUM | - | Forwarding and consolidation summary message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 22 |  | Next Segment

SG15 | - | C | 9999 | - | CNI-DTM-CNT-TSR-MOA-FTX-SG21-SG22-SG30-SG37-SG56
CNI | - | M | 1 | - | Consignment information
Function:
To identify one consignment.
EDIFACT
EAN
*
Description |
1490
Consolidation item number
C |  | n..4
R
C503
DOCUMENT/MESSAGE DETAILS
C |
O
| 1004
| Document/message number |
C |  | an..35
R
Consignor shipment reference number. |
| 1373
| Document/message status, coded |
C |  | an..3
N
| 1366
| Document/message source |
C |  | an..35
N
| 3453
| Language, coded |
C |  | an..3
N
1312
Consignment load sequence number
C |  | n..4
O
Segment Notes:
This segment is used to identify a consignment included in the consolidation by its shipment reference number. In the IFTMnn messages the shipment reference number is provided in data element 1153 of the RFF segment at the message level using the code value 'CU'. DE 1490: Serial number differentiating each separate consignment included in the consolidation. DE 1312: This data element is used to indicate the sequence in which a consignment is to be loaded in a consolidation. Example : CNI+12+AVV23441'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |