EANCOM PART II |  | 1997-07-01

IFCSUM | - | Forwarding and consolidation summary message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 6 |  | Next Segment

SG1 | - | C | 9 | - | RFF-DTM
RFF | - | M | 1 | - | Reference
Function:
To specify a reference.
EDIFACT
EAN
*
Description |
C506
REFERENCE
M |
M
| 1153
| Reference qualifier |
M |  | an..3
M
*
ACD = Additional reference number
CT = Contract number
CU = Consignor's reference number
PFB = Firm booking reference number (EAN Code)
PK = Packing list number
SRN = Shipment reference number
TRI = Transport instruction number (EAN Code)
| 1154
| Reference number |
C |  | an..35
R
| 1156
| Line number |
C |  | an..6
N
| 4000
| Reference version number |
C |  | an..35
N
Segment Notes:
This segment is used to specify references which are related to the complete message. DE 1153: Code values 'PFB' and 'TRI' should only be used in conjunction with the codes 1 or 5 in data element 1225 in the BGM segment. DE 1153: Code value 'CU' is used to provide references generated by the consignor which are relevant for the complete consolidation. Example : RFF+TRI:6214'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |