EANCOM PART II |  | 1997-07-01

INSDES | - | Instruction to despatch | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 18 |  | Next Segment

SG10 | - | C | 9999 | - | LIN-PIA-IMD-QTY-GIN-DTM-FTX-MOA-SG11-SG12-SG13
LIN | - | M | 1 | - | Line item
Function:
To identify a line item and configuration.
EDIFACT
EAN
*
Description |
1082
Line item number
C |  | n..6
R
Application generated number of the item lines within the instruction to despatch.
1229
Action request/notification, coded
C |  | an..3
N
C212
ITEM NUMBER IDENTIFICATION
C |
D
| 7140
| Item number |
C |  | an..35
R
Format n..14 EAN-8, UPC-A, EAN-13, or DUN-14 - this is the number of the article being despatched. |
| 7143
| Item number type, coded |
C |  | an..3
R
*
EN = International Article Numbering Association (EAN)
UP = UPC (Universal product code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
C829
SUB-LINE INFORMATION
C |
D
| 5495
| Sub-line indicator, coded |
C |  | an..3
R
| 1082
| Line item number |
C |  | n..6
R
1222
Configuration level
C |  | n..2
N
7083
Configuration, coded
C |  | an..3
N
Segment Notes:
This segment is used to identify the line item for which instructions for despatch are being provided. Note: If the instruction to despatch is being provided for a full package (e.g. pallet) containing one or more products which have been allocated a serial shipping container code then only the line item number (data element 1082) should be provided in the LIN segment. The serial shipping container code to identify the full package should be specified in the GIN segment (number 22). Note: Should it be required to provide the SSCC marked on the packaging of the article identified in the LIN segment then the GIN segment in group 13 should be used. Example : LIN+1++5412345123453:EN' Instruction to despatch the product identified by the EAN article number 5412345123453. LIN+2' No article number provided, serial shipping container code specified in the GIN segment at line level. Dependency Notes : C212: This composite is only used for the identification of EAN/UPC articles codes. If another coding structure (other than serial shipping container codes) is required, e.g. harmonised system, this composite will not be used and the code will be detailed in the PIA segment. DE's C829 and 7083: These data elements are only used when sub-lines are required. FOR A COMPLETE DESCRIPTION ON THE USAGE OF SUB-LINES PLEASE REFER TO PART I, SECTION 4.11 .

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |