EANCOM PART II |  | 1997-07-01

IFTMIN | - | Instruction message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 43 |  | Next Segment

SG18 | - | C | 999 | - | GID-HAN-TMP-RNG-LOC-MOA-PIA-FTX-SG19-SG20-SG21-SG22-SG23-SG24-SG29-SG32
SG32 | - | C | 9 | - | DGS-FTX-SG33-SG34
DGS | - | M | 1 | - | Dangerous goods
Function:
To identify dangerous goods.
EDIFACT
EAN
*
Description |
8273
Dangerous goods regulations, coded
C |  | an..3
R
ADR = European agreement regarding the total carriage of dangerous goods
CFR = 49 code of federal regulations
ICA = IATA ICAO
RID = Rail/road dangerous goods book (RID)
C205
HAZARD CODE
C |
O
| 8351
| Hazard code identification |
M |  | an..7
M
| 8078
| Hazard substance/item/page number |
C |  | an..7
O
| 8092
| Hazard code version number |
C |  | an..10
O
C234
UNDG INFORMATION
C |
O
| 7124
| UNDG number |
C |  | n4
O
| 7088
| Dangerous goods flashpoint |
C |  | an..8
O
C223
DANGEROUS GOODS SHIPMENT FLASHPOINT
C |
O
| 7106
| Shipment flashpoint |
C |  | n3
O
| 6411
| Measure unit qualifier |
C |  | an..3
O
8339
Packing group, coded
C |  | an..3
O
1 = Great danger
2 = Medium danger
3 = Minor danger
8364
EMS number
C |  | an..6
O
8410
MFAG
C |  | an..4
O
8126
Trem card number
C |  | an..10
O
C235
HAZARD IDENTIFICATION
C |
N
| 8158
| Hazard identification number, upper part |
C |  | an..4
| 8186
| Substance identification number, lower part |
C |  | an4
C236
DANGEROUS GOODS LABEL
C |
N
| 8246
| Dangerous goods label marking |
C |  | an..4
| 8246
| Dangerous goods label marking |
C |  | an..4
| 8246
| Dangerous goods label marking |
C |  | an..4
8255
Packing instruction, coded
C |  | an..3
N
8325
Category of means of transport, coded
C |  | an..3
N
8211
Permission for transport, coded
C |  | an..3
N
Segment Notes:
This segment is used to indicate whether the goods item contains any dangerous goods. Example : DGS+ADR+3B+1178+021:CEL'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |