EANCOM PART II |  | 1997-07-01

IFTMBF | - | Firm booking message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 35 |  | Next Segment

SG32 | - | C | 999 | - | EQD-EQN-SG33
EQD | - | M | 1 | - | Equipment details
Function:
To identify a unit of equipment.
EDIFACT
EAN
*
Description |
8053
Equipment qualifier
M |  | an..3
M
BPN = Box pallet non exchangeable
CN = Container
EFP = Exchangeable EUR flat pallet
PA = Pallet
UL = ULD (Unit load device)
C237
EQUIPMENT IDENTIFICATION
C |
R
| 8260
| Equipment identification number |
C |  | an..17
O
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
9 = EAN (International Article Numbering association)
| 3207
| Country, coded |
C |  | an..3
O
C224
EQUIPMENT SIZE AND TYPE
C |
O
| 8155
| Equipment size and type identification |
C |  | an..10
O
6 = Pressurized tank
21 = Container IC 20 ft.
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
| 8154
| Equipment size and type |
C |  | an..35
O
8077
Equipment supplier, coded
C |  | an..3
O
1 = Shipper supplied
2 = Carrier supplied
8249
Equipment status, coded
C |  | an..3
N
8169
Full/empty indicator, coded
C |  | an..3
O
4 = Empty
5 = Full
Segment Notes:
This segment is used to indicate the units of equipment which will be used to transport the goods items specified. DE 8260: The positioning of goods items within equipment in a consignment is controlled through a link with the SGP segment using the DE 8260. DE 8260 in the EQD segment should have the same value as that specified in the SGP segment (DE 8260) in the applicable goods item group to establish the link. Example : EQD+UL+45223'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |