EANCOM PART II |  | 1997-07-01
QALITY | - Quality Test Report Message | VERSION 001

## 6. Example

The following is an example of a Quality message sent on the 15th of June 1996 by the testing party Stockholm Meter Service to the party, identified by the EAN location number 5412345123453, who ordered the test.

The message which is identified by the number 45223, provides test results for a meter according to the test specification number 52114.

UNH+ME000001+QALITY:D:96A:UN:EAN001' | Message header
BGM+4+45223+9' | Quality message number 45223
DTM+137:19960615:102' | Message date 15th June 1996
RFF+TS:52114' | Test specification number 52114
NAD+OB+5412345123453::9' | Ordering party identified by EAN location number 5412345123453
NAD+TPE+++STOCKHOLM METER SERVICES' | Testing party Stockholm Meter Services
CTA+IC+:BJORN NIELSEN' | Testing party contact person
COM+031-13425:TE' | Telephone number for contact person
COM+031-13455:FX' | Fax number for contact person
LIN+1++5412345111115:EN' | Identification of the test carried out for the article identified by the EAN code 5412345111115
PIA+5+SE-OSC-K135:SA::91' | Identification of meter type using supplier allocated number
PIA+1+SVM93:MF::90' | Identification of the manufacturers article number
PIA+1+9216995:SN::91' | Identification of meter serial number
IMD+F++:::PROTOCOL OF METER:CONTROL DATA' | Description of the test
MEA+SV+AAU+CEL::20:150' | Specification of operating temperature range in celsius
DTM+94:19950212:102' | Meter manufactured on the 12th of February 1995
QTY+79:17108:MWH' | Previous meter read 17108 megawatt hours
QTY+79:34608:MTQ' | Previous meter read 34608 cubic metres
QTY+74:17119:MWH' | Latest meter read 17119 megawatt hours
QTY+74:34641:MTQ' | Latest meter read 34641 cubic metres
NAD+MF+++SVM' | Identification of the manufacturer of the meter
CCI+TES' | Indication of start of first test results
MEA+MV+TC+CEL::50:50' | Test measured value in temperature range of 50-50 degrees celsius
MEA+TR+ENE+MWH:0.5' | Test results = energy efficiency of 0.5 megawatt hours
CCI+TES' | Indication of start of second test results
MEA+MV+TC+CEL::50:49' | Test measured value in temperature range of 50-49 degrees celsius
MEA+TR+ENE+MWH:47.6' | Test results = energy efficiency of 47.6 megawatt hours
CCI+TES' | Indication of start of third test results
MEA+MV+TC+CEL::73:70' | Test measured value in temperature range of 73-70 degrees celsius
MEA+TR+ENE+MWH:140.8' | Test results = energy efficiency of 140.8 megawatt hours
CCI+TES' | Indication of start of fourth test results
MEA+MV+TC+CEL::67:60' | Test measured value in temperature range of 67-60 degrees celsius
MEA+TR+ENE+MWH:328.9' | Test results = energy efficiency of 328.9 megawatt hours
CCI+TES' | Indication of start of fifth test results
MEA+MV+TC+CEL::73:60' | Test measured value in temperature range of 73-60 degrees celsius
MEA+TR+ENE+MWH:610.8’ | Test results = energy efficiency of 610.8 megawatt hours
UNT+37+ME000001' | Message trailer - 37 segments in the message

Note :
The EDI interchange will include the UNB...UNZ segments and, if applicable, the UNG...UNE segments (see Part 1, section 2.7)

(c) Copyright EAN 1997