EANCOM PART II |  | 1997-07-01

PRODAT | - | Product data message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 43 |  | Next Segment

SG8 | - | M | 999 | - | LIN-PIA-DTM-MEA-HAN-DOC-FTX-PGI-SG9-SG10-SG12-SG14-SG15-SG16-SG17-SG19-SG20-SG21
SG20 | - | C | 5 | - | PAC-MEA-HAN-PCI
PCI | - | C | 5 | - | Package identification
Function:
To specify markings and labels on individual packages or physical units.
EDIFACT
EAN
*
Description |
4233
Marking instructions, coded
C |  | an..3
O
30 = Mark serial shipping container code
C210
MARKS & LABELS
C |
O
| 7102
| Shipping marks |
M |  | an..35
M
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
8275
Container/package status, coded
C |  | an..3
N
C827
TYPE OF MARKING
C |
N
| 7511
| Type of marking, coded |
M |  | an..3
| 1131
| Code list qualifier |
C |  | an..3
| 3055
| Code list responsible agency, coded |
C |  | an..3
Segment Notes:
This segment is used to specify what marks and labels will appear on the packaging identified in the PAC segment. Example : PCI+30'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |