EANCOM PART III DATA ELEMENT & CODE SETS DIRECTORY |  | 1997-07-01

Previous Data Element |  | Next Data Element

8169
| Full/empty indicator, coded
| To indicate the extent to which the equipment is full or empty.

| 1
= | More than one quarter volume available
| 2
= | More than half volume available
| Self explanatory.
| 4
= | Empty
| 5
= | Full
| 6
= | No volume available
| Self explanatory.

Previous Data Element |  | Next Data Element

(c) Copyright EAN 1997 |