EANCOM PART II |  | 1997-07-01

DESADV | - | Despatch advice message | VERSION | 005

5. Segments Layout |

Previous Segment |  | Segment number: | 45 |  | Next Segment

SG10 | - | C | 9999 | - | CPS-SG11-SG15
SG15 | - | C | 9999 | - | LIN-PIA-IMD-MEA-QTY-DLM-DTM-FTX-SG16-SG18-SG20-SG23
SG20 | - | C | 9999 | - | PCI-DTM-MEA-QTY-SG21-SG22
SG22 | - | C | 10 | - | HAN
HAN | - | M | 1 | - | Handling instructions
Function:
To specify handling and where necessary, notify hazards.
EDIFACT
EAN
*
Description |
C524
HANDLING INSTRUCTIONS
C |
R
| 4079
| Handling instructions, coded |
C |  | an..3
R
BIG = Outsized
CRU = Crushable (EAN Code)
EAT = Foodstuffs
HWC = Handle with care (EAN Code)
PSC = Pest controlling (EAN Code)
STR = Stacking restricted (EAN Code)
UST = Unstackable (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
D
*
9 = EAN (International Article Numbering association)
| 4078
| Handling instructions |
C |  | an..70
O
C218
HAZARDOUS MATERIAL
C |
O
| 7419
| Hazardous material class code, identification |
C |  | an..4
O
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
Segment Notes:
This segment is used to provide handling instructions relevant to the packaging unit and level described in the PCI segment. Example : HAN+EAT' Dependency Notes : DE 3055: This data element is only used when codes PSC, CRU, UST, HWC or STR are used in data element 4079.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |