EANCOM PART II |  | 1997-07-01

ORDCHG | - | Purchase order change request message | VERSION | 005

5. Segments Layout |

Previous Segment |  | Segment number: | 72 |  | Next Segment

SG26 | - | C | 200000 | - | LIN-PIA-IMD-MEA-QTY-DTM-MOA-GIN-QVR-FTX-SG30-SG31-SG32-SG35-SG36-SG37-SG41-SG47
SG41 | - | C | 99 | - | ALC-ALI-DTM-SG42-SG43-SG44-SG45-SG46
SG43 | - | C | 1 | - | PCD-RNG
RNG | - | C | 1 | - | Range details
Function:
To identify a range.
EDIFACT
EAN
*
Description |
6167
Range type qualifier
M |  | an..3
M
1 = Allowance range
2 = Charge range
C280
RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
PCE = Piece
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
Segment Notes:
This segment is used to specify ranges which apply to the previous PCD segment. Example : RNG+1+PCE:200:800'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |