EANCOM PART II |  | 1997-07-01

HANMOV | - | Cargo/goods handling and movement message | VERSION | 002

4. Segments Description |

UNH | - | M | 1 | - | MESSAGE HEADER
This segment is used to head, identify and specify a message.
BGM | - | M | 1 | - | Beginning of message
This segment is used to indicate the type and function of a message and to transmit the identifying number.
DTM | - | C | 9 | - | Date/time/period
This segment is used to specify the date of the cargo/goods handling and movement message.
HAN | - | C | 9 | - | Handling instructions
This segment is used to provide handling instructions, and where necessary to provide hazardous information, relevant to the complete cargo/goods handling and movement message.
FTX | - | C | 9 | - | Free text
This segment is used to indicate free text information related to the entire message.
SG2 | - | C | 9 | - | RFF-DTM
A group of segments containing references and constants which apply to the entire message.
RFF | - | M | 1 | - | Reference
This segment is used to specify references which relate to the whole cargo/goods handling and movement message, for example, contract number.
DTM | - | C | 9 | - | Date/time/period
This segment is used to specify dates relating to the references given in the previous RFF segment.
SG3 | - | C | 9 | - | NAD-LOC-SG4
A group of segments to identify a party, related references, locations, contacts and required documents.
NAD | - | M | 1 | - | Name and address
This segment is used to identify the parties involved in the Cargo/goods handling and movement process. Identification of the service ordering party (e.g. buyer, supplier, etc) and the logistic service provider is mandatory in the message.
LOC | - | C | 9 | - | Place/location identification
This segment is used to identify locations relevant to the parties identified in the NAD segment.
SG4 | - | C | 9 | - | RFF
A group of segments to specify a reference related to the party.
RFF | - | M | 1 | - | Reference
This segment is used to specify reference numbers related to the trading parties identified in the previous NAD segment.
Cargo/Goods Handling And Movement Detail Section
SG7 | - | C | 99 | - | LIN-PIA-IMD-HAN-SG8-QTY-DTM-FTX-SG10-SG11
A group of segments providing details of the individually handled product items.
LIN | - | M | 1 | - | Line item
This segment is used to signify the beginning of the detail section of the cargo/goods handling and movement message. The detail section is formed by a repeating group of segments, always starting with a LIN segment.
PIA | - | C | 9 | - | Additional product id
This segment is used to specify additional or substitutional item identification codes such as a buyer's or supplier's item number.
IMD | - | C | 99 | - | Item description
This segment is used to provide description of the current line item.
HAN | - | C | 9 | - | Handling instructions
This segment is used to provide handling instructions, and where necessary to provide hazardous information, relevant to the current line item.
SG8 | - | C | 9 | - | NAD
A group of segments for identifying names and addresses and their functions.
NAD | - | M | 1 | - | Name and address
This segment is used to identify parties related to the current line item. It may be used as an aid to product selection, e.g. all products from one manufacturer, or as information which is to be used when preparing a shipment containing the product, e.g. carrier, delivery party, etc.
QTY | - | C | 9 | - | Quantity
This segment is used to specify quantities related to the current line item.
DTM | - | C | 9 | - | Date/time/period
This segment is used to specify dates related to the current line item. Dates specified here may be used as an aid to product selection, e.g. destroy all products with sell by date greater than 1st of January 1997.
FTX | - | C | 9 | - | Free text
This segment is used to indicate free text information related to the current line item.
SG10 | - | C | 9 | - | RFF
A group of segments to give reference numbers and dates.
RFF | - | M | 1 | - | Reference
This segment is used to provide references specific to the line item. References specified here override any global references provided in the heading section of the cargo/goods handling and movement message when the same qualifier is used.
SG11 | - | C | 99 | - | PAC-MEA-QTY-SG12
A group of segments providing details how the product item is packed, such as number and type of packages, physical measurements and quantities.
PAC | - | M | 1 | - | Package
This segment is used to specify the packaging details for the currently identified line item.
MEA | - | C | 9 | - | Measurements
This segment is used to provide measurements relevant to the packaging described in the PAC segment.
QTY | - | C | 9 | - | Quantity
This segment is used to specify the quantity per package specified in the PAC segment.
SG12 | - | C | 9 | - | PCI-GIN
A group of segments identifying one specific package or a number of packages, their marks and numbers.
PCI | - | M | 1 | - | Package identification
This segment is used to provide markings and labels information relevant to the packaging identified in the PAC segment.
GIN | - | C | 9 | - | Goods identity number
This segment is used to provide identification numbers relevant to the packaging identified in the PAC segment.
Cargo/Goods Handling And Movement Summary Section
UNT | - | M | 1 | - | MESSAGE TRAILER
This segment is a mandatory UN/EDIFACT segment. It must always be the last segment in the message.

(c) Copyright EAN 1997 |