EANCOM PART II |  | 1997-07-01

CREMUL | - | Multiple credit advice message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 22 |  | Next Segment

SG4 | - | M | 9999 | - | LIN-DTM-BUS-MOA-SG5-SG6-SG7-SG10
SG10 | - | M | 9999 | - | SEQ-DTM-BUS-FII-SG11-SG12-SG13-SG14-SG15-SG16-SG17-SG20
SEQ | - | M | 1 | - | Sequence details
Function:
To provide specific details related to the delivery sequence.
EDIFACT
EAN
*
Description |
1245
Status indicator, coded
C |  | an..3
N
C286
SEQUENCE INFORMATION
C |
R
| 1050
| Sequence number |
M |  | an..6
M
| 1159
| Sequence number source, coded |
C |  | an..3
N
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
N
Segment Notes:
This segment is used to identify the start of the specification of individual transactions (level C) by means of a sequence number within the current line number. The sequence number should be reset to one for each occurrence of a new line number (in LIN segment). Example : SEQ++1'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |