EANCOM PART II |  | 1997-07-01

IFTMBF | - | Firm booking message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 11 |  | Next Segment

SG7 | - | C | 99 | - | TDT-DTM-SG8
TDT | - | M | 1 | - | Details of transport
Function:
To specify the transport details such as mode of transport, means of transport, its conveyance reference number and the identification of the means of transport.
EDIFACT
EAN
*
Description |
8051
Transport stage qualifier
M |  | an..3
M
10 = Pre-carriage transport
20 = Main-carriage transport
30 = On-carriage transport
8028
Conveyance reference number
C |  | an..17
O
Reference number covering the transport
C220
MODE OF TRANSPORT
C |
R
| 8067
| Mode of transport, coded |
C |  | an..3
R
10 = Maritime transport
20 = Rail transport
30 = Road transport
40 = Air transport
60 = Multimodal transport
| 8066
| Mode of transport |
C |  | an..17
N
C228
TRANSPORT MEANS
C |
O
| 8179
| Type of means of transport identification |
C |  | an..8
D
23 = Rail bulk car
25 = Rail express
31 = Truck
| 8178
| Type of means of transport |
C |  | an..17
D
C040
CARRIER
C |
O
| 3127
| Carrier identification |
C |  | an..17
A
EAN Location Number - Format n13 |
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
A
9 = EAN (International Article Numbering association)
| 3128
| Carrier name |
C |  | an..35
O
8101
Transit direction, coded
C |  | an..3
N
C401
EXCESS TRANSPORTATION INFORMATION
C |
N
| 8457
| Excess transportation reason, coded |
M |  | an..3
| 8459
| Excess transportation responsibility, coded |
M |  | an..3
| 7130
| Customer authorization number |
C |  | an..17
C222
TRANSPORT IDENTIFICATION
C |
O
| 8213
| Id. of means of transport identification |
C |  | an..9
O
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
| 8212
| Id. of the means of transport |
C |  | an..35
R
Vehicle license plate/Aircraft number. |
| 8453
| Nationality of means of transport, coded |
C |  | an..3
O
ISO 3166 two alpha code |
8281
Transport ownership, coded
C |  | an..3
N
Segment Notes:
This segment is used to indicate the transport means, and where necessary, the carrier to be used for the consignment being booked. When used, it is mandatory to indicate the main carriage transport mode in this segment. Example : TDT+20++30+31' Dependency Notes : Data Elements 8179 and 8178 are only used when the type of means of transport must be specifically identified, that is, a generic description such as road transport is unsuitable.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |