EANCOM PART II |  | 1997-07-01

IFTSTA | - | International multimodal status report message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 7 |  | Next Segment

SG4 | - | C | 999 | - | CNI-SG5
CNI | - | M | 1 | - | Consignment information
Function:
To identify one consignment.
EDIFACT
EAN
*
Description |
1490
Consolidation item number
C |  | n..4
R
C503
DOCUMENT/MESSAGE DETAILS
C |
R
| 1004
| Document/message number |
C |  | an..35
R
Consignor's shipment reference number |
| 1373
| Document/message status, coded |
C |  | an..3
N
| 1366
| Document/message source |
C |  | an..35
N
| 3453
| Language, coded |
C |  | an..3
N
1312
Consignment load sequence number
C |  | n..4
O
Segment Notes:
This segment is used to identify a consignment for which status information is being provided. In the IFTMnn messages the consignor's shipment reference number is provided in data element 1153 of the RFF segment at the message level using the code value 'CU'. DE 1490: Serial number differentiating each separate consignment included in the status report. DE 1312: This data element is used to indicate the sequence in which a consignment is to be, or has been, loaded. Example : CNI+12+AVV23441'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |