EANCOM PART II |  | 1997-07-01

PAYMUL | - | Multiple payment order message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 40 |  | Next Segment

SG4 | - | M | 9999 | - | LIN-DTM-RFF-BUS-FCA-SG5-SG6-SG7-SG8-SG9-SG10-SG11
SG11 | - | M | 9999 | - | SEQ-MOA-DTM-RFF-PAI-FCA-SG12-SG13-SG14-SG15-SG16
SG13 | - | C | 3 | - | NAD-CTA-COM
COM | - | C | 5 | - | Communication contact
Function:
To identify a communication number of a department or a person to whom communication should be directed.
EDIFACT
EAN
*
Description |
C076
COMMUNICATION CONTACT
M |
M
| 3148
| Communication number |
M |  | an..512
M
| 3155
| Communication channel qualifier |
M |  | an..3
M
*
CA = Cable address
EI = EDI
EM = Electronic mail
FX = Fax
TE = Telephone
TL = Telex
Segment Notes:
This segment is used to provide communications details relevant to the contact identified in the CTA segment. Example : COM+003212187674:FX'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |