EANCOM PART II |  | 1997-07-01

HANMOV | - | Cargo/goods handling and movement message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 2 |  | Next Segment

BGM | - | M | 1 | - | Beginning of message
Function:
To indicate the type and function of a message and to transmit the identifying number.
EDIFACT
EAN
*
Description |
C002
DOCUMENT/MESSAGE NAME
C |
R
| 1001
| Document/message name, coded |
C |  | an..3
R
*
90E = Cargo/goods handling and movement message (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
R
*
9 = EAN (International Article Numbering association)
| 1000
| Document/message name |
C |  | an..35
O
1004
Document/message number
C |  | an..35
R
Cargo/goods handling and movement number assigned by document sender.
1225
Message function, coded
C |  | an..3
R
*
1 = Cancellation
5 = Replace
9 = Original
31 = Copy
4343
Response type, coded
C |  | an..3
N
Segment Notes:
This segment is used to indicate the type and function of a message and to transmit the identifying number. It is recommended that the length of the document number be restricted to a maximum of 17 characters. DE 1225: The message function, coded is a critical data element in this segment. It applies to all data indicated in the message. The following definitions apply for the restricted codes: 1 = Cancellation - A previous handling and movement notice is being cancelled. Only the mandatory segments in the message along with the NAD segments identifying the sender and recipient need to be re-transmitted. Identification of the previously sent message should take place in the RFF segment in group 2. 5 = Replacement - The current message cancels and replaces a previously sent handling and movement message. Identification of the previously sent message should take place in the RFF segment in group 2. 9 = Original - An original transmission of an handling and movement message. 31 = Copy - A copy of an handling and movement message for a third party for information purposes. The identification of the message being copied should be provided in data element 1004. Example : BGM+90E::9+WH3212+9'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |