EANCOM PART II |  | 1997-07-01

RECADV | - | Receiving advice message | VERSION | 003

5. Segments Layout |

Previous Segment |  | Segment number: | 2 |  | Next Segment

BGM | - | M | 1 | - | Beginning of message
Function:
To indicate the type and function of a message and to transmit the identifying number.
EDIFACT
EAN
*
Description |
C002
DOCUMENT/MESSAGE NAME
C |
R
| 1001
| Document/message name, coded |
C |  | an..3
R
*
352 = Receiving advice (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
R
*
9 = EAN (International Article Numbering association)
| 1000
| Document/message name |
C |  | an..35
O
1004
Document/message number
C |  | an..35
R
Receiving Advice number assigned by the document sender.
1225
Message function, coded
C |  | an..3
R
*
5 = Replace
9 = Original
4343
Response type, coded
C |  | an..3
N
Segment Notes:
This segment is used to indicate the type and function of a message and to transmit the identifying number. All references other than the document message number DE 1004 are to be put into the RFF segment. DE 1004: It is recommended that the length of the document number be restricted to a maximum of 17 characters. DE 1225: The message function coded, is a critical data element in this segment. It applies to all data indicated in the message. The following definitions apply for the restricted codes: 5 = Replace - This code indicates that the current receiving advice message is a replacement due to an error in a previous message. The previous message should be identified in the RFF segment group 1. 9 = Original - An original transmission of a Receiving Advice. Example : BGM+352::9+REC5488+9'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |