EANCOM PART II |  | 1997-07-01

IFTSTA | - | International multimodal status report message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 9 |  | Next Segment

SG4 | - | C | 999 | - | CNI-SG5
SG5 | - | M | 99 | - | STS-RFF-DTM-FTX-NAD-LOC-SG9
RFF | - | C | 9 | - | Reference
Function:
To specify a reference.
EDIFACT
EAN
*
Description |
C506
REFERENCE
M |
M
| 1153
| Reference qualifier |
M |  | an..3
M
AAS = Transport document number
AAU = Despatch note number
ALO = Receiving advice number
BM = Bill of lading number
CT = Contract number
CU = Consignor's reference number
DQ = Delivery note number
FF = Freight forwarder's reference number
| 1154
| Reference number |
C |  | an..35
R
| 1156
| Line number |
C |  | an..6
O
| 4000
| Reference version number |
C |  | an..35
N
Segment Notes:
This segment is used to identify any reference associated with the status information in the STS segment. Example : RFF+SRN:6532'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |