EANCOM PART II |  | 1997-07-01

RECADV | - | Receiving advice message | VERSION | 003

5. Segments Layout |

Previous Segment |  | Segment number: | 21 |  | Next Segment

SG16 | - | C | 9999 | - | CPS-SG17-SG22
SG22 | - | C | 9999 | - | LIN-PIA-QTY-QVR-DTM-SG28-SG29
SG28 | - | C | 10 | - | RFF-DTM
RFF | - | M | 1 | - | Reference
Function:
To specify a reference.
EDIFACT
EAN
*
Description |
C506
REFERENCE
M |
M
| 1153
| Reference qualifier |
M |  | an..3
M
AAK = Despatch advice number
AAU = Despatch note number
ALO = Receiving advice number
CR = Customer reference number
ON = Order number (buyer)
POR = Purchase order response number
PP = Purchase order change number
VN = Order number (supplier)
| 1154
| Reference number |
C |  | an..35
R
| 1156
| Line number |
C |  | an..6
O
| 4000
| Reference version number |
C |  | an..35
N
Segment Notes:
This segment is used to specify any references associated with the current line item. Example : RFF+AAK:63321'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |