EANCOM PART II |  | 1997-07-01

DESADV | - | Despatch advice message | VERSION | 005

5. Segments Layout |

Previous Segment |  | Segment number: | 38 |  | Next Segment

SG10 | - | C | 9999 | - | CPS-SG11-SG15
SG15 | - | C | 9999 | - | LIN-PIA-IMD-MEA-QTY-DLM-DTM-FTX-SG16-SG18-SG20-SG23
SG18 | - | C | 100 | - | LOC-DTM-QTY
QTY | - | C | 10 | - | Quantity
Function:
To specify a pertinent quantity.
EDIFACT
EAN
*
Description |
C186
QUANTITY DETAILS
M |
M
| 6063
| Quantity qualifier |
M |  | an..3
M
*
11 = Split quantity
12 = Despatch quantity
| 6060
| Quantity |
M |  | n..15
M
| 6411
| Measure unit qualifier |
C |  | an..3
D
KGM = Kilogram
Segment Notes:
This segment is used to indicate the delivery quantity for the delivery location specified in the previous LOC segment. The total of all quantities specified in segment group 18 for the line must equal the value for the total quantity detailed in the QTY segment at line level. Example : QTY+11:14' Dependency Notes : DE 6411: This DE is only used if the product being despatched is a variable quantity product.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |