EANCOM PART II |  | 1997-07-01

INVRPT | - | Inventory report message | VERSION | 004

5. Segments Layout |

Previous Segment |  | Segment number: | 12 |  | Next Segment

SG9 | - | C | 9999 | - | LIN-PIA-IMD-SG11
LIN | - | M | 1 | - | Line item
Function:
To identify a line item and configuration.
EDIFACT
EAN
*
Description |
1082
Line item number
C |  | n..6
R
Application generated number of the count of the item lines within the Inventory Report.
1229
Action request/notification, coded
C |  | an..3
N
C212
ITEM NUMBER IDENTIFICATION
C |
R
| 7140
| Item number |
C |  | an..35
R
Format n..14 EAN-8, UPC-A, EAN-13, or DUN-14 - this is the number of the article being reported. |
| 7143
| Item number type, coded |
C |  | an..3
R
*
EN = International Article Numbering Association (EAN)
UP = UPC (Universal product code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
C829
SUB-LINE INFORMATION
C |
D
| 5495
| Sub-line indicator, coded |
C |  | an..3
R
*
1 = Sub-line information
| 1082
| Line item number |
C |  | n..6
R
1222
Configuration level
C |  | n..2
N
7083
Configuration, coded
C |  | an..3
D
A = Added to the configuration
D = Deleted from the configuration
I = Included in the configuration
Segment Notes:
This segment is used to identify a specific line item in the inventory report. The detail section of the Inventory Report is formed by a repeating group of segments, always starting with the LIN segment. In a simple Inventory Report covering one location, the LIN segment will contain the product identification with related stock quantities specified using only the QTY and LOC segments in segment group 11. In an extended Inventory Report covering multiple locations, an available option is to provide total stock quantities for all locations using the QTY and LOC segments in segment group 11, with the quantities per location further broken down using the full range of segments available in segment group 11. Example : LIN+1++5412345111115:EN' Dependency Notes : DE C829 and 7083: These data elements are only used when sub-lines are required. FOR A COMPLETE DESCRIPTION ON THE USAGE OF SUB-LINES PLEASE REFER TO PART I, SECTION 4.11.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |