EANCOM PART II |  | 1997-07-01

RECADV | - | Receiving advice message | VERSION | 003

5. Segments Layout |

Previous Segment |  | Segment number: | 24 |  | Next Segment

SG16 | - | C | 9999 | - | CPS-SG17-SG22
SG22 | - | C | 9999 | - | LIN-PIA-QTY-QVR-DTM-SG28-SG29
SG29 | - | C | 9999 | - | PCI-QTY-QVR-SG31
QTY | - | C | 1 | - | Quantity
Function:
To specify a pertinent quantity.
EDIFACT
EAN
*
Description |
C186
QUANTITY DETAILS
M |
M
| 6063
| Quantity qualifier |
M |  | an..3
M
*
194 = Received and accepted
| 6060
| Quantity |
M |  | n..15
M
| 6411
| Measure unit qualifier |
C |  | an..3
D
Segment Notes:
This segment is used to indicate the quantity of the current line item received and accepted which is contained in the package marked with the Serial Shipping Container Code identified in the following GIN segment. Example : QTY+194:45' Dependency Note : DE 6411: This DE is only used if the current product is of variable quantity.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |