EANCOM PART II |  | 1997-07-01

PAYMUL | - | Multiple payment order message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 44 |  | Next Segment

SG4 | - | M | 9999 | - | LIN-DTM-RFF-BUS-FCA-SG5-SG6-SG7-SG8-SG9-SG10-SG11
SG11 | - | M | 9999 | - | SEQ-MOA-DTM-RFF-PAI-FCA-SG12-SG13-SG14-SG15-SG16
SG15 | - | C | 10 | - | GIS-MOA-LOC-NAD-RCS-FTX
GIS | - | M | 1 | - | General indicator
Function:
To transmit a processing indicator.
EDIFACT
EAN
*
Description |
C529
PROCESSING INDICATOR
M |
M
| 7365
| Processing indicator, coded |
M |  | an..3
M
*
10 = Declaration requested
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
N
| 7187
| Process type identification |
C |  | an..17
N
Segment Notes:
This segment is used to indicate that the information contained in the following segments will be passed on to and processed by the central and regulatory party identified in the NAD segment. This segment should not be used if the GIS segment in segment group 9 has already been used. Note: The use of this segment group is subject to domestic regulations stipulated by regulatory authorities, e.g. Central Bank. Example : GIS+10'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |