EANCOM PART II |  | 1997-07-01

INSDES | - | Instruction to despatch | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 22 |  | Next Segment

SG10 | - | C | 9999 | - | LIN-PIA-IMD-QTY-GIN-DTM-FTX-MOA-SG11-SG12-SG13
GIN | - | C | 99 | - | Goods identity number
Function:
To give specific identification numbers, either as single numbers or ranges.
EDIFACT
EAN
*
Description |
7405
Identity number qualifier
M |  | an..3
M
*
BJ = Serial shipping container code
C208
IDENTITY NUMBER RANGE
M |
M
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
C208
IDENTITY NUMBER RANGE
C |
N
| 7402
| Identity number |
M |  | an..35
| 7402
| Identity number |
C |  | an..35
C208
IDENTITY NUMBER RANGE
C |
N
| 7402
| Identity number |
M |  | an..35
| 7402
| Identity number |
C |  | an..35
C208
IDENTITY NUMBER RANGE
C |
N
| 7402
| Identity number |
M |  | an..35
| 7402
| Identity number |
C |  | an..35
C208
IDENTITY NUMBER RANGE
C |
N
| 7402
| Identity number |
M |  | an..35
| 7402
| Identity number |
C |  | an..35
Segment Notes:
This segment is used to provide SSCC codes for identification purposes only. If used, this segment may be repeated only once per occurance of segment group 10 (LIN) to provide the SSCC as the primary means of identification. Note: If a serial shipping container is identified in this segment then no product identification should be provided in composite C212 of the LIN segment. Example : GIN+BJ+354123450000000014' Despatch the package identified by the serial shipping container code 354123450000000014.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |