EANCOM PART II |  | 1997-07-01

IFTMIN | - | Instruction message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 10 |  | Next Segment

SG3 | - | C | 99 | - | RFF-DTM
RFF | - | M | 1 | - | Reference
Function:
To specify a reference.
EDIFACT
EAN
*
Description |
C506
REFERENCE
M |
M
| 1153
| Reference qualifier |
M |  | an..3
M
AWB = Air waybill number
BN = Booking reference number
CT = Contract number
CU = Consignor's reference number
HWB = House waybill number
LC = Letter of credit number
MWB = Master air waybill number
TRI = Transport instruction number (EAN Code)
| 1154
| Reference number |
C |  | an..35
R
| 1156
| Line number |
C |  | an..6
N
| 4000
| Reference version number |
C |  | an..35
N
Segment Notes:
This segment is used to specify references related to the complete transport instruction message. DE 1153: Code value 'TRI' is only used when codes values 1 (Cancellation) or 5 (Replacement) are used in data element 1225 of the BGM segment. The code value 'CU' is the common reference number for the consignment which is used in all transport messages (IFTMBF, IFTMIN, IFTMAN, etc). Example : RFF+CT:76214'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |