EANCOM PART II |  | 1997-07-01

PROINQ | - | Product inquiry message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 19 |  | Next Segment

SG4 | - | M | 9999 | - | LIN-SG5-SG6
SG6 | - | C | 9999 | - | IRQ-PIA-MEA-NAD-PGI-DTM-SG7
SG7 | - | C | 9 | - | PRI-RNG
RNG | - | C | 1 | - | Range details
Function:
To identify a range.
EDIFACT
EAN
*
Description |
6167
Range type qualifier
M |  | an..3
M
3 = Monetary range
C280
RANGE
C |
R
| 6411
| Measure unit qualifier |
M |  | an..3
M
AMT = Amount (EAN Code)
KGM = Kilogram
PCE = Piece
| 6162
| Range minimum |
C |  | n..18
O
| 6152
| Range maximum |
C |  | n..18
O
Segment Notes:
This segment is used to specify price ranges for the current line item. The type of price for which the range is required is specified in the previous PRI segment. The message sender would use this segment to request only information for products which fall within the specified range. Example : RNG+3+AMT:1500:4000' The message sender requests information on products which fall between the 1500 and 4000 BF price range.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |