EANCOM PART II |  | 1997-07-01

ORDERS | - | Purchase order message | VERSION | 008

5. Segments Layout |

Previous Segment |  | Segment number: | 57 |  | Next Segment

SG25 | - | C | 200000 | - | LIN-PIA-IMD-MEA-QTY-DTM-MOA-GIN-QVR-FTX-SG28-SG29-SG30-SG33-SG34-SG35-SG39-SG45
SG30 | - | C | 10 | - | PAC-SG32
SG32 | - | C | 5 | - | PCI-RFF-DTM-GIN
GIN | - | C | 10 | - | Goods identity number
Function:
To give specific identification numbers, either as single numbers or ranges.
EDIFACT
EAN
*
Description |
7405
Identity number qualifier
M |  | an..3
M
*
BJ = Serial shipping container code
BN = Serial number
BX = Batch number
EU = EAN / UPC number (EAN Code)
C208
IDENTITY NUMBER RANGE
M |
M
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
O
Segment Notes:
This segment is used to indicate numbers which are to be marked on packages for the line items in the message. Example : GIN+BJ+354123450000000014:354123450000000106'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |