EANCOM PART II |  | 1997-07-01
HANMOV | - Cargo/Goods Handling and Movement Message | VERSION 002

## 6. Examples

### Example 6

The following is an example of a Cargo/goods handling and movement message sent from a supplier identified by the EAN location number 5422331123459 to his logistic service provider identified by the EAN location number 5432154111113. The message is dated the 14th of January 1997 and has the message reference WH5155.

The message requests the logistic services provider to first pick 12 units of the product identified by the EAN article number 5412345111184 from the returnable pallet identified by the EAN SSCC 354107380000001051 and to pack them on the pallet type ISO 1 and to label this pallet with the EAN SSCC 354123450000000106.

Next, 20 units of the product identified by the EAN article number 4000862141404 are to be picked from the returnable pallet identified by the EAN SSCC 354123450000000014 and packed on the ISO 1 pallet identified by the EAN SSCC 354123450000000106 on top of the first product loaded on this pallet.

Finally, 10 units of the product identified by the EAN article number 4000862141411 are to be taken from the returnable pallet identified by the EAN SSCC 354107380000001068 and put on a 1/8 Euro pallet. This pallet is to be labelled with the EAN SSCC 354123451234567892 and the original article number, 4000862141411, of the product.

EAN Article Number | Qty | From pallet type | From pallet SSCC | To pallet type | To pallet SSCC
4000862141404 | 20 | Return | 354123450000000014 | ISO 1 | 354123450000000106
5412345111184 | 12 | Return | 354107380000001051 | ISO 1 | 354123450000000106
4000862141411 | 10 | Return | 354107380000001068 | 1/8 Euro | 354123451234567892

UNH+1+HANMOV:D:96A:EN:EAN002' | Message header
BGM+90E::9+WH5155+9' | Cargo/goods handling and movement number WH6222
DTM+137:19970114:102' | Message date 14th of January 1997
HAN+UNP::9' | Message requests un-packing service
HAN+PKS::9' | and pick in sequence service
HAN+PAC::9' | and packing service
HAN+LAB::9' | and labelling service
NAD+SU+5422331123459::9' | Supplier is identified by the EAN location number 5422331123459
NAD+LSP+5432154111113::9' | Logistic service provider is identified by the EAN location number 5432154111113
LIN+1++5412345111184:EN' | First product to be picked is identified by the EAN article number 5412345111184
QTY+1:12' | 12 units subject to the instruction
PAC+1+::1E+09::9' | Are to be un-packed from one returnable pallet
QTY+52:12' | Quantity per pack is 12
PCI+33E' | The pallet is marked with a Serial Shipping Container Code
GIN+BJ+354107380000001051' | Serial Shipping Container Code 354107380000001051 is marked on package
PAC+1+::3E+201::9' | Are to be packed in one ISO 1 pallet
QTY+52:12' | Quantity per pack is 12
PCI+33E' | The pallet is marked with a Serial Shipping Container Code
GIN+BJ+354123450000000106' | Serial Shipping Container Code is marked on package 354123450000000106
LIN+2++4000862141404:EN' | Second product to be picked is identified by the EAN article number 4000862141404
QTY+1:20' | 20 units subject to the instruction
PAC+1+::1E+09::9' | Are to be un-packed from one returnable pallet
QTY+52:20' | Quantity per pack is 20
PCI+33E' | The pallet is marked with a Serial Shipping Container Code
GIN+BJ+354123450000000014' | Serial Shipping Container Code 354123450000000014 is marked on package
PAC+1+::3E+201::9' | Are to be packed in one ISO 1 pallet
QTY+52:20' | Quantity per pack is 20
PCI+30' | The pallet is to be marked with a Serial Shipping Container Code
GIN+BJ+354123450000000106' | Serial Shipping Container Code 354123450000000106 is to be marked on package
LIN+3++4000862141411:EN' | Third product to be picked is identified by the EAN article number 4000862141411
QTY+1:10' | 10 units subject to the instruction
PAC+1+::1E+09::9' | Are to be un-packed from one returnable pallet
QTY+52:10' | Quantity per pack is 10
PCI+33E' | The pallet is marked with a Serial Shipping Container Code
GIN+BJ+354107380000001068' | Serial Shipping Container Code 354107380000001068 is marked on package
PAC+1+::3E+204::9' | Are to be packed in one 1/8 Euro pallet
QTY+52:10' | Quantity per pack is 10
PCI+30' | The pallet is to be marked with a Serial Shipping Container Code
GIN+BJ+354123451234567892' | Serial Shipping Container Code 354123451234567892 is to be marked on package
PCI+32E' | The pallet is also to be marked with an EAN/UPC number
GIN+EU+4000862141411' | EAN/UPC number 4000862141411 is to be marked on package
UNT+42+1' | Message trailer - 42 segments in the message

Note :
The EDI interchange will include the UNB..UNZ segments and, if applicable, the UNG..UNE segments. (See part 1 section 2.7).

(c) Copyright EAN 1997