EANCOM PART II |  | 1997-07-01

DESADV | - | Despatch advice message | VERSION | 005

5. Segments Layout |

Previous Segment |  | Segment number: | 48 |  | Next Segment

CNT | - | C | 5 | - | Control total
Function:
To provide control total.
EDIFACT
EAN
*
Description |
C270
CONTROL
M |
M
| 6069
| Control qualifier |
M |  | an..3
M
*
1 = Total value of the quantity segments at line level in a message
2 = Number of line items in message
7 = Total gross weight
11 = Total number of packages
29 = Total net weight of consignment
| 6066
| Control value |
M |  | n..18
M
| 6411
| Measure unit qualifier |
C |  | an..3
O
Segment Notes:
This segment is used to provide message control information for checking on the message receiver's in-house system. DE 6069: When using code value '7= Total gross weight' in this data element the total specified in data element 6066 is arrived at by adding the values in data element 6314 of the MEA segment at LIN level when code value AAB is used in the same MEA segment. When using code value '11= Total number of packages' in this data element the total specified in data element 6066 is arrived at by adding the values in data element 7224 of the PAC segments in the messages. When using code value '29 = Total net weight of consignment' in this data element the total specified in data element 6066 is arrived at by adding the values in data element 6314 of the MEA segment at LIN level when code value AAA is used in the same MEA segment. Example : CNT+2:12'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |