EANCOM PART III DATA ELEMENT & CODE SETS DIRECTORY |  | 1997-07-01

Previous Data Element |  | Next Data Element

6155
| Measurement attribute, coded
| Code used to specify non-discrete measurement values.

@ | 42
= | Uncontrolled temperature
| Uncontrolled temperature conditions.
40E |
@ | 43
= | Chilled
| Somewhere between four degrees Celsius and twelve degrees Celsius.
41E |
@ | 44
= | Frozen
| Less than zero degrees Celsius.
42E |
@ | 45
= | Temperature controlled
| Required temperature value.
43E |

Previous Data Element |  | Next Data Element

(c) Copyright EAN 1997 |