EANCOM PART II |  | 1997-07-01

RECADV | - | Receiving advice message | VERSION | 003

5. Segments Layout |

Previous Segment |  | Segment number: | 14 |  | Next Segment

SG16 | - | C | 9999 | - | CPS-SG17-SG22
SG17 | - | C | 9999 | - | PAC-QVR-SG18
SG18 | - | C | 999 | - | PCI-SG20
PCI | - | M | 1 | - | Package identification
Function:
To specify markings and labels on individual packages or physical units.
EDIFACT
EAN
*
Description |
4233
Marking instructions, coded
C |  | an..3
R
17 = Supplier's instructions
33E = Marked with serial shipping container code (EAN Code)
C210
MARKS & LABELS
C |
O
| 7102
| Shipping marks |
M |  | an..35
M
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
| 7102
| Shipping marks |
C |  | an..35
O
8275
Container/package status, coded
C |  | an..3
N
C827
TYPE OF MARKING
C |
N
| 7511
| Type of marking, coded |
M |  | an..3
| 1131
| Code list qualifier |
C |  | an..3
| 3055
| Code list responsible agency, coded |
C |  | an..3
Segment Notes:
This segment is used to provide markings and labels information relevant to the packaging unit identified in the PAC segment. The segment may be used to provide labelling information on shipping containers not known by the receiver of the goods. Example : PCI+17+CONTAINER ABN54421'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |