EANCOM PART II |  | 1997-07-01

RETINS | - | Returns instruction | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 13 |  | Next Segment

SG6 | - | C | 99 | - | CDI-DTM-FTX
CDI | - | C | 1 | - | Physical or logical state
Function:
To describe a physical or logical state.
EDIFACT
EAN
*
Description |
7001
Physical or logical state qualifier
M |  | an..3
M
3E = Upon return (EAN Code)
C564
PHYSICAL OR LOGICAL STATE INFORMATION
M |
M
| 7007
| Physical or logical state, coded |
C |  | an..3
A
12E = Return goods (EAN Code)
13E = Dispose of goods (EAN Code)
14E = Destroy goods (EAN Code)
15E = Repair goods (EAN Code)
16E = Hold for examination (EAN Code)
17E = Return refused (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
9 = EAN (International Article Numbering association)
| 7006
| Physical or logical state |
C |  | an..35
O
Segment Notes:
This segment is used to indicate conditions specified by the message sender concerning the return or otherwise of all the goods detailed in the message. Example: CDI+3E+13E::9' All of the goods detailed in the message should be disposed of.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |