EANCOM PART II |  | 1997-07-01

MSCONS | - | Metered services consumption report | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 27 |  | Next Segment

SG5 | - | M | 99999 | - | NAD-SG6
SG6 | - | M | 99999 | - | LOC-DTM-SG7-SG8-SG9
SG9 | - | C | 99999 | - | LIN-PIA-IMD-PRI-NAD-MOA-SG10-SG11
SG11 | - | C | 99 | - | CCI-MEA-DTM
CCI | - | M | 1 | - | Characteristic/class id
Function:
To identify and describe a specific characteristic.
EDIFACT
EAN
*
Description |
7059
Property class, coded
C |  | an..3
O
PCM = Product characteristic (EAN Code)
C502
MEASUREMENT DETAILS
C |
N
| 6313
| Measurement dimension, coded |
C |  | an..3
| 6321
| Measurement significance, coded |
C |  | an..3
| 6155
| Measurement attribute, coded |
C |  | an..3
| 6154
| Measurement attribute |
C |  | an..70
C240
PRODUCT CHARACTERISTIC
C |
O
| 7037
| Characteristic identification |
M |  | an..17
M
| 1131
| Code list qualifier |
C |  | an..3
M
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
91 = Assigned by supplier or supplier's agent
92 = Assigned by buyer or buyer's agent
60 = Assigned by national trade agency
| 7036
| Characteristic |
C |  | an..35
O
| 7036
| Characteristic |
C |  | an..35
O
Segment Notes:
This segment is used to specify the characteristics of the current line item. DE 7037: This data element is used to identify the characteristics of the current line item in coded form. As no EDIFACT code list exists for this data element codes should be allocated depending on the requirements of the user. Should it not be possible to provide a user code in this data element and a free form characteristic description is used in data element 7036, then it is recommended that the code value ‘ZZZ’ be put in data element 7037 (which is mandatory). DE 7036: This data element is used to provide free form text characteristics for use where no coded values exist in data element 7037. Example 1 : CCI+PCM++82::91' This example indicates for the gas industry that the characteristic being identified for the product is calorific value through the use of the supplier assigned code value 82.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |