EANCOM PART II |  | 1997-07-01

PRODAT | - | Product data message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 47 |  | Next Segment

SG8 | - | M | 999 | - | LIN-PIA-DTM-MEA-HAN-DOC-FTX-PGI-SG9-SG10-SG12-SG14-SG15-SG16-SG17-SG19-SG20-SG21
SG21 | - | C | 999 | - | HYN-QTY-SG23
SG23 | - | C | 99 | - | CCI-CAV-MEA
CAV | - | C | 10 | - | Characteristic value
Function:
To provide the value of a characteristic.
EDIFACT
EAN
*
Description |
C889
CHARACTERISTIC VALUE
M |
M
| 7111
| Characteristic value, coded |
C |  | an..3
A
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
9 = EAN (International Article Numbering association)
60 = Assigned by national trade agency
91 = Assigned by supplier or supplier's agent
92 = Assigned by buyer or buyer's agent
| 7110
| Characteristic value |
C |  | an..35
O
| 7110
| Characteristic value |
C |  | an..35
O
Segment Notes:
This segment is used to further specify characteristic for the current hierarchy. DE 7111: This data element is used to provide characteristic values. As no EDIFACT code list exists for this data element codes should be allocated depending on the requirements of the user. Example: CAV+22::91' When used in combination with the CCI segment example, the supplier code 22 indicates the fact that there is a 386 chip in the system control board.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |