EANCOM PART II |  | 1997-07-01

IFTMAN | - | Arrival notice message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 35 |  | Next Segment

SG18 | - | C | 999 | - | GID-TMP-RNG-FTX-SG19-SG20-SG21-SG22-SG23-SG27-SG30
SG30 | - | C | 9 | - | DGS-FTX-SG31-SG32
SG31 | - | C | 9 | - | CTA-COM
COM | - | C | 9 | - | Communication contact
Function:
To identify a communication number of a department or a person to whom communication should be directed.
EDIFACT
EAN
*
Description |
C076
COMMUNICATION CONTACT
M |
M
| 3148
| Communication number |
M |  | an..512
M
| 3155
| Communication channel qualifier |
M |  | an..3
M
EM = Electronic mail
FX = Fax
TE = Telephone
TL = Telex
XF = X.400
Segment Notes:
This segment identifies the communications number and type of communications for the person or department identified in the preceding CTA segment. Example : COM+0033148759632:TE'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |