EANCOM PART II |  | 1997-07-01

IFTSTA | - | International multimodal status report message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 16 |  | Next Segment

SG4 | - | C | 999 | - | CNI-SG5
SG5 | - | M | 99 | - | STS-RFF-DTM-FTX-NAD-LOC-SG9
SG9 | - | C | 99 | - | GID-SG12
SG12 | - | C | 99 | - | PCI-GIN
GIN | - | C | 9 | - | Goods identity number
Function:
To give specific identification numbers, either as single numbers or ranges.
EDIFACT
EAN
*
Description |
7405
Identity number qualifier
M |  | an..3
M
*
BJ = Serial shipping container code
C208
IDENTITY NUMBER RANGE
M |
M
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
C208
IDENTITY NUMBER RANGE
C |
O
| 7402
| Identity number |
M |  | an..35
M
| 7402
| Identity number |
C |  | an..35
N
Segment Notes:
This segment is used to provide the Serial Shipping Container Code marked on the packaging of the current goods item. In EANCOM it is required to use the Serial Shipping Container Code (SSCC's) for unique identification of individual transport packages. Example : GIN+BJ+354123450000000014'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |