EANCOM PART II |  | 1997-07-01

PRICAT | - | Price/sales catalogue message | VERSION | 006

5. Segments Layout |

Previous Segment |  | Segment number: | 74 |  | Next Segment

SG16 | - | C | 1000 | - | PGI-DTM-QTY-ALI-FTX-SG17-SG18-SG19-SG20-SG26-SG29-SG30-SG31-SG32-SG33
SG33 | - | C | 999999 | - | LIN-PIA-IMD-MEA-QTY-HAN-ALI-DTM-RFF-LOC-FTX-SG35-SG37-SG38-SG44-SG45
HAN | - | C | 5 | - | Handling instructions
Function:
To specify handling and where necessary, notify hazards.
EDIFACT
EAN
*
Description |
C524
HANDLING INSTRUCTIONS
C |
| 4079
| Handling instructions, coded |
C |  | an..3
R
BIG = Outsized
CRU = Crushable (EAN Code)
DAE = Dangerous article (EAN Code)
EAT = Foodstuffs
FTD = Frost danger (EAN Code)
HWC = Handle with care (EAN Code)
LYG = Lying
PSC = Pest controlling (EAN Code)
SSN = Smell sensitive (EAN Code)
STK = Stackable
STR = Stacking restricted (EAN Code)
TDR = Transit or cross docking delivery
UPR = Up right/standing
UST = Unstackable (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
D
2 = CEC (Commission of the European Communities)
9 = EAN (International Article Numbering association)
| 4078
| Handling instructions |
C |  | an..70
O
C218
HAZARDOUS MATERIAL
C |
O
| 7419
| Hazardous material class code, identification |
C |  | an..4
O
| 1131
| Code list qualifier |
C |  | an..3
O
ADR = Accord Europeen relatif au transport international des marchandises
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
Segment Notes:
This segment is used to specify any handling instructions for the current line item. Handling instructions related to the packaging of the product are provided in the HAN segment of the PAC segment group. Example : HAN+EAT' Dependency Notes : DE 3055: This data element must be used when using any of the EAN specific codes in data element 4079, e.g., HWC, STR, etc.

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |