EANCOM PART II |  | 1997-07-01

IFTMIN | - | Instruction message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 7 |  | Next Segment

CNT | - | C | 9 | - | Control total
Function:
To provide control total.
EDIFACT
EAN
*
Description |
C270
CONTROL
M |
M
| 6069
| Control qualifier |
M |  | an..3
M
7 = Total gross weight
11 = Total number of packages
15 = Total consignment, cube
16 = Total number of equipment
| 6066
| Control value |
M |  | n..18
M
| 6411
| Measure unit qualifier |
C |  | an..3
O
Segment Notes:
This segment is used to provide message control information such as the total weight of the consignment, or, the total number of items in the consignment. DE 6069: When using value '15' in this data element the total specified in data element 6066 is arrived at by adding the values specified in data element 6314 of the MEA segment at goods item level when the GMC (Gross measurement cube) code is used in data element 6313 in the same MEA segment. When using code value '11' the total specified in data element 6066 is arrived at by adding the values specified only in the first occurrence of C213, data element 7224, of the GID segment. Example : CNT+11:4'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |