EANCOM PART II |  | 1997-07-01

IFTMIN | - | Instruction message | VERSION | 001

5. Segments Layout |

Previous Segment |  | Segment number: | 52 |  | Next Segment

SG37 | - | C | 999 | - | EQD-MEA-DIM-SEL-SG39
SEL | - | C | 99 | - | Seal number
Function:
To specify a seal number related to equipment.
EDIFACT
EAN
*
Description |
9308
Seal number
M |  | an..10
M
C215
SEAL ISSUER
C |
R
| 9303
| Sealing party, coded |
C |  | an..3
R
CA = Carrier
CU = Customs
SH = Shipper
| 1131
| Code list qualifier |
C |  | an..3
O
| 3055
| Code list responsible agency, coded |
C |  | an..3
O
| 9302
| Sealing party |
C |  | an..35
O
4517
Seal condition, coded
C |  | an..3
O
Segment Notes:
This segment is used to specify a seal number for the equipment identified in the EQD segment. Example : SEL+96753+SH'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |