EANCOM PART II |  | 1997-07-01

OSTRPT | - | Order status report | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 9 |  | Next Segment

SG3 | - | C | 1000 | - | DOC-DTM-SG4-SG5
DOC | - | M | 1 | - | Document/message details
Function:
To identify documents, either printed, electronically transferred, or referenced as specified in message description, including, where relevant, the identification of the type of transaction that will result from this message.
EDIFACT
EAN
*
Description |
C002
DOCUMENT/MESSAGE NAME
M |
M
| 1001
| Document/message name, coded |
C |  | an..3
R
220 = Order
221 = Blanket order
226 = Call off order
351 = Despatch advice
80E = Instruction to despatch (EAN Code)
90E = Cargo/goods handling and movement message (EAN Code)
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
N
| 1000
| Document/message name |
C |  | an..35
N
C503
DOCUMENT/MESSAGE DETAILS
C |
R
| 1004
| Document/message number |
C |  | an..35
R
| 1373
| Document/message status, coded |
C |  | an..3
N
| 1366
| Document/message source |
C |  | an..35
N
| 3453
| Language, coded |
C |  | an..3
N
3153
Communication channel identifier, coded
C |  | an..3
N
1220
Number of copies of document required
C |  | n..2
N
1218
Number of originals of document required
C |  | n..2
N
Segment Notes:
This segment is used to identify the document(s) for which status information is being provided. Example : DOC+220+OR877-22'

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |