EANCOM PART II |  | 1997-07-01

IFTSTA | - | International multimodal status report message | VERSION | 002

5. Segments Layout |

Previous Segment |  | Segment number: | 4 |  | Next Segment

SG1 | - | C | 9 | - | NAD
NAD | - | M | 1 | - | Name and address
Function:
To specify the name/address and their related function, either by CO82 only and/or structured by CO80 thru 3207.
EDIFACT
EAN
*
Description |
3035
Party qualifier
M |  | an..3
M
CA = Carrier
CN = Consignee
CZ = Consignor
FW = Freight forwarder
C082
PARTY IDENTIFICATION DETAILS
C |
A
| 3039
| Party id. identification |
M |  | an..35
M
EAN Location number - Format n13 |
| 1131
| Code list qualifier |
C |  | an..3
N
| 3055
| Code list responsible agency, coded |
C |  | an..3
R
*
9 = EAN (International Article Numbering association)
C058
NAME AND ADDRESS
C |
N
| 3124
| Name and address line |
M |  | an..35
| 3124
| Name and address line |
C |  | an..35
| 3124
| Name and address line |
C |  | an..35
| 3124
| Name and address line |
C |  | an..35
| 3124
| Name and address line |
C |  | an..35
C080
PARTY NAME
C |
D
| 3036
| Party name |
M |  | an..35
M
Party Name, clear text |
| 3036
| Party name |
C |  | an..35
O
| 3036
| Party name |
C |  | an..35
O
| 3036
| Party name |
C |  | an..35
O
| 3036
| Party name |
C |  | an..35
O
| 3045
| Party name format, coded |
C |  | an..3
O
C059
STREET
C |
D
| 3042
| Street and number/p.o. box |
M |  | an..35
M
Building Name/Number and Street |
| 3042
| Street and number/p.o. box |
C |  | an..35
O
Name and/or P.O. Box |
| 3042
| Street and number/p.o. box |
C |  | an..35
O
| 3042
| Street and number/p.o. box |
C |  | an..35
O
3164
City name
C |  | an..35
D
City/Town, clear text
3229
Country sub-entity identification
C |  | an..9
D
County/State, clear text
3251
Postcode identification
C |  | an..9
D
Postal Code
3207
Country, coded
C |  | an..3
D
ISO 3166 two alpha code
Segment Notes:
This segment is used to identify the trading partners involved in the Transport Status message. Identification of the Consignor and Consignee is mandatory in the transport status message. If required, a carrier or freight forwarder may also be identified using NAD at this level in the message. For the identification of parties it is recommended to use EAN location Numbers. If coded address information can not be used it is recommended to use a structured address (C080 through 3207). Example : NAD+CN+5411234512309::9' NAD+CZ+5412345123453::9' Dependency Notes : The following composites and data elements are only used when a coded name and address can not be used. The affected composites and data elements are as follows: C080 - C059 - 3164 - 3229 - 3251 - 3207

Previous Segment |  | Next Segment

(c) Copyright EAN 1997 |